,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##other##,Voltage##other##,Body & Trim Finish##other##,Photometric Web File##other##
AX20-J4-K0-F20-U2,4000,1900,120,Metal - Betacalco - Silver Metallic,AX20-J4.ies
AX20-J3-K0-F20-U2,3500,1805,120,Metal - Betacalco - Silver Metallic,AX20-J4.ies
AX20-J2-K0-F20-U2,3000,1767,120,Metal - Betacalco - Silver Metallic,AX20-J4.ies
AX20-J4-K0-F2-U2,4000,1900,120,Metal - Betacalco - Black,AX20-J4.ies
AX20-J3-K0-F2-U2,3500,1805,120,Metal - Betacalco - Black,AX20-J4.ies
AX20-J2-K0-F2-U2,3000,1767,120,Metal - Betacalco - Black,AX20-J4.ies
AX20-J4-K0-F1-U2,4000,1900,120,Metal - Betacalco - White,AX20-J4.ies
AX20-J3-K0-F1-U2,3500,1805,120,Metal - Betacalco - White,AX20-J4.ies
AX20-J2-K0-F1-U2,3000,1767,120,Metal - Betacalco - White,AX20-J4.ies
AX20-J4-K0-F27-U2,4000,1900,120,Metal - Betacalco - Light Cherry,AX20-J4.ies
AX20-J3-K0-F27-U2,3500,1805,120,Metal - Betacalco - Light Cherry,AX20-J4.ies
AX20-J2-K0-F27-U2,3000,1767,120,Metal - Betacalco - Light Cherry,AX20-J4.ies
AX20-J4-K0-F28-U2,4000,1900,120,Metal - Betacalco - Dark Walnut,AX20-J4.ies
AX20-J3-K0-F28-U2,3500,1805,120,Metal - Betacalco - Dark Walnut,AX20-J4.ies
AX20-J2-K0-F28-U2,3000,1767,120,Metal - Betacalco - Dark Walnut,AX20-J4.ies
