,"Diameter 18""##other##","Diameter 24""##other##","Diameter 36""##other##",Direct##other##,Input Wattage Direct##other##,Input Wattage Indirect##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##other##,Voltage##other##,Fixture Finish##other##,Photometric Web File##other##
TMRP1P01-LMA0170-CR80-CTA40,1,0,0,1,16,0,4000,1719,120,Metal - Betacalco - Black Metallic,TMRP1P01-LMA0170-CR80-CTA40.ies
TMRP1P01-LMA0250-CR80-CTA40,1,0,0,1,25,0,4000,2529,120,Metal - Betacalco - Black Metallic,TMRP1P01-LMA0250-CR80-CTA40.ies
TMRP1P01-LMA0320-CR80-CTA40,1,0,0,1,34,0,4000,3185,120,Metal - Betacalco - Black Metallic,TMRP1P01-LMA0320-CR80-CTA40.ies
TMRP1P02-LMA0320-CR80-CTA40,0,1,0,1,28,0,4000,3147,120,Metal - Betacalco - Black Metallic,TMRP1P02-LMA0320-CR80-CTA40.ies
TMRP1P02-LMA0420-CR80-CTA40,0,1,0,1,38,0,4000,4149,120,Metal - Betacalco - Black Metallic,TMRP1P02-LMA0420-CR80-CTA40.ies
TMRP1P02-LMA0530-CR80-CTA40,0,1,0,1,51,0,4000,5273,120,Metal - Betacalco - Black Metallic,TMRP1P02-LMA0530-CR80-CTA40.ies
TMRP1P03-LMA0730-CR80-CTA40,0,0,1,1,63,0,4000,7342,120,Metal - Betacalco - Black Metallic,TMRP1P03-LMA0730-CR80-CTA40.ies
TMRP1P03-LMA1060-CR80-CTA40,0,0,1,1,98,0,4000,10606,120,Metal - Betacalco - Black Metallic,TMRP1P03-LMA1060-CR80-CTA40.ies
TMRP1P03-LMA1300-CR80-CTA40,0,0,1,1,132,0,4000,13429,120,Metal - Betacalco - Black Metallic,TMRP1P03-LMA1300-CR80-CTA40.ies
TMRP1P04-LMA1300-CR80-CTA40,0,0,0,1,112,0,4000,12937,120,Metal - Betacalco - Black Metallic,TMRP1P04-LMA1300-CR80-CTA40.ies
TMRP1P04-LMA1900-CR80-CTA40,0,0,0,1,178,0,4000,19066,120,Metal - Betacalco - Black Metallic,TMRP1P04-LMA1900-CR80-CTA40.ies
TMRP1P04-LMA2400-CR80-CTA40,0,0,0,1,239,0,4000,24008,120,Metal - Betacalco - Black Metallic,TMRP1P04-LMA2400-CR80-CTA40.ies
TMRP2P01-LMA0170-LMB0120-CR80-CTA40-CTB40,1,0,0,0,16,9.9,4000,1719,120,Metal - Betacalco - Black Metallic,TMRP1P01-LMA0170-CR80-CTA40.ies
