,"Diameter 18""##other##",Input Wattage##other##,Luminous Flux##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Body Finish##other##,Photometric Web File##other##
WHPP1P18-CR80-CTA40-FA01-DL00,1,22.4,3262,4000,Metal - Betacalco - White,WHPP1P18-CR80-CTA40-FA01-DL00.ies
WHPP1P24-CR80-CTA40-FA01-DL00,0,33.6,4873,4000,Metal - Betacalco - White,WHPP1P24-CR80-CTA40-FA01-DL00.ies
WHPP1P18-CR80-CTA40-FA01-DL40,1,50,5217,4000,Metal - Betacalco - White,WHPP1P18-CR80-CTA40-FA01-DL40.ies
WHPP1P24-CR80-CTA40-FA01-DL40,0,61.2,6723,4000,Metal - Betacalco - White,WHPP1P24-CR80-CTA40-FA01-DL40.ies
